**METAL CORE-RACK**

**Superior construction !**

**Core-shack capacity :**

**NQ:**

* 315 boxes per side x 2 = 630 boxes of 15’ of core = 9450 » (2881m) of core

**BQ**

* 315 boxes per side x 2 = 630 boxes x 20’ of core = 12 600’ (3841m) of core.

**Size:**

* Lenght: 10’
* Width: 8’
* Height: 8’ (roofing including)

**Roof:** Galvanized aluminium 28 gauge.

**Trust:** 1/8’’ thick with rods of 9/16’’ of diameter.

**Structure:** ¼’’ thick with rods of 9/16’’ of diameter.

This core rack can store up to 42 boxes more than any similar model**.**

**Our metal core rack is the only engineer certified design on the market**